 //Copyright 2009 - 2010 Intel Corporation All Rights Reserved.
 #pragma namespace("\\\\.\\root")

instance of __Namespace {
	name="Intel_ME";
};

#pragma namespace("\\\\.\\root\\Intel_ME")
  [Version ( "0.0.1" ), 
    Description ( "A class providing access to Intel(R) AMT Features configuration, such as KVM and IDE-Redirect" )
:Amended, LOCALE(0x409), dynamic: ToInstance, provider("IntelMEProv")]
class AMT_Service : CIM_Service {
	[Description ("Indicates whether the WebUI capability is currently enabled"): Amended, static, implemented]
	uint32 isWebUIEnabled([OUT] boolean enabled);
	[Description ("Indicates whether SOL is currently enabled / active"): Amended, static, implemented]
	uint32 getSOLState(
		[OUT, Description("Indicates whether SOL is enabled by MEBX"), 
		ValueMap { "0", "1", "2"},  
		Values { "Enabled", "Disabled", "UNKNOWN" }] 
		UINT32 hardEnabled, 
		[OUT, Description("Indicates whether SOL is enabled by WS-Management interface (using AMT_RedirectionService class)"), 
		ValueMap { "0", "1", "2"},  
		Values { "Enabled", "Disabled", "UNKNOWN" }] 
		UINT32 softEnabled, 
		[OUT, Description("Indicates whether SOL session is currently open")] 
		boolean active);
	[Description ("Indicates whether IDER is currently enabled / active"): Amended, static, implemented]
	uint32 getIDERState(
		[OUT, Description("Indicates whether IDER is enabled by MEBX"), 
		ValueMap { "0", "1", "2"},  
		Values { "Enabled", "Disabled", "UNKNOWN" }] 
		UINT32 hardEnabled, 
		[OUT, Description("Indicates whether IDER is enabled by WS-Management interface (using AMT_RedirectionService class)"), 
		ValueMap { "0", "1", "2"},  
		Values { "Enabled", "Disabled", "UNKNOWN" }] 
		UINT32 softEnabled, 
		[OUT, Description("Indicates whether IDER session is currently open")] 
		boolean active);
	[Description ("Indicates whether KVM is currently enabled / active"): Amended, static, implemented]
	uint32 getKVMState(
		[OUT, Description("Indicates whether KVM is enabled by MEBX"), 
		ValueMap { "0", "1", "2"},  
		Values { "Enabled", "Disabled", "UNKNOWN" }] 
		UINT32 hardEnabled, 
		[OUT, Description("Indicates whether KVM is enabled by WS-Management interface (using CIM_KVMRedirectionSAP class)"),
		ValueMap { "0", "1", "2"},  
		Values { "Enabled", "Disabled", "UNKNOWN" }] 
		UINT32 softEnabled, 
		[OUT, Description("Indicates whether KVM session is currently open")] 
		boolean active);
	[Description ("Terminates KVM session"): Amended, static, implemented]
	uint32 TerminateKVMSession();
	[Description("Allows user to specify Sprite zoom level: No zoom: 1 Zoom x2: 2"): Amended, static, implemented]
	uint32 setSpriteZoom([IN, ValueMap { "1", "2"}, 
	       Values { "No zoom", "Zoom x2"} ] uint8 zoom);
	[Description("Allows user to specify Sprite locale"): Amended, static, implemented]
	uint32 setSpriteLocale([IN, ValueMap {"0","1","2","3","4","5","6","7","8","9","10"}, Values { "English", "French", "German", "Chinese Traditional", "Japanese", "Russian","Italian", "Spanish", "Portuguese Brazil", "Korean", "Chinese Simplified"}] uint8 locale);
};
