 //Copyright 2009 - 2010 Intel Corporation All Rights Reserved.
#pragma namespace("\\\\.\\root")

instance of __Namespace {
	name="Intel_ME";
};

#pragma namespace("\\\\.\\root\\Intel_ME")

[Version ( "0.0.4" ), 
    Description ( "A class Representing Intel(R) Manageability Engine (Intel(R) ME) information" ):Amended, dynamic: ToInstance, provider("IntelMEProv"):ToInstance]
class ME_System : CIM_ComputerSystem {
   
   [ Description ("Intel(R) ME firmware version in format: Major.Minor.Revision.build")]
   string FWVersion; 

	[Description ("Capabilities represents the supported features on this system"),
      bitValues { "AMT", "Irwt", "iQST", "TDT", "SoftCreek", "VE", "DT", 
		"NAND", "MPC", "ICCOverClocking", "PAVP", "SPK", "RCA", "RPAT", "IPv6", "KVM", "Och", 
		"VLan", "TLS", "CILA", "StdMng", "L3"}]
   uint32 Capabilities;	


	[Description ("EnabledCapabilities represents the enabled features on this system"),
      bitValues {"AMT", "Irwt", "iQST", "TDT", "SoftCreek", "VE", "DT", 
		"NAND", "MPC", "ICCOverClocking", "PAVP", "SPK", "RCA", "RPAT", "IPv6", "KVM", "Och", 
		"VLan", "TLS", "CILA", "StdMng", "L3"}]
   uint32 EnabledCapabilities;	

	[Description ("PlatformType represents the category the system belongs to"),
      	ValueMap { "0", "1", "2", "3"},
		Values { "Mobile", "Desktop", "Server", "Workstation" }]
   uint32 PlatformType;

	[Description ("UserSegmentType represents the market segment the system belongs to"),
		ValueMap { "0", "1"},
		Values { "Corporate", "Consumer" }]
   uint32 UserSegmentType;

	[Description ("ManageabilityMode represents the manageability mode. Every mode supports a different set of capabilities"),
		ValueMap { "0", "1", "2", "3"},
		Values { "None", "Unknown", "vPro", "Standard Manageability" }]
   uint32 ManageabilityMode;
	

      [Description ( "Represents the status of the chipset CryptoFuse, when disabled, Intel(R) ME will not perform any encryption operations" )]
   boolean CryptoFuseEnabled;
   
   [Description ( "Receives local  FW Update counters (In Intel(R) AMT version 7.0 and later this function is not supported and always returns NOT SUPPORTED error)")  : Amended, static, implemented]
   uint32 getFwUpdateOverrideParams(
   		[OUT, Description ("FW Update override counter. When 255 refer to always"),
		ValueMap {"0", "1...254", "255"}] uint32 Counter, 
   		[OUT, Description ("FW Update override qualifier"),
   		ValueMap { "0", "1", "2" }, 
	        Values { "ALWAYS", "NEVER", "RESTRICTED"}] uint32 OverrideQualifier); 
   
   [Description("Returns the cause for the last Intel(R) ME Reset operation"): Amended, static, implemented]
   uint32 getLastMEResetReason(
	[OUT, Description("A description of the last Intel(R) ME reset reason"), 
	ValueMap { "0", "1", "2", "3" }, 
       Values { "Power-Up", "FW-Reset", "System-Reset", "Unknown" }]
	uint32 ReasonCode);
   
	[Description ("Specifies the list of ACPI states Intel(R) ME is operational in"): Amended, static, implemented]  
   uint32 getCurrentPowerPolicy(
	   [OUT, Description("A description of the power policy")]
	   string PowerPolicy);

 [Description ("Indicates whether the Firmware Update capability is currently enabled"): Amended, static, implemented]
  uint32 IsFirmwareUpdateEnabled([OUT] boolean enabled);

[Description ("Specifies the list of supported features on this system"): Amended, static, implemented]  
   uint32 getCapabilities(
	   [OUT, Description("An array of strings defining system capabilities. Should match the bitvalues of the system Capabilities")]
	   string Capabilities[],
	   [OUT, Description("An array of strings defining system capabilities. Should match the bitvalues of the system Enabled Capabilities")]
	   string EnabledCapabilities[]);

	  	
};
