// Copyright (c) 2005 DMTF.  All rights reserved.
// <change cr="ArchCR00066.004" type="add">Add UmlPackagePath
// qualifier values to CIM Schema.</change>
// ==================================================================
//  CIM_MemoryMappedIO 
// ==================================================================
   [Version ( "2.6.0" ), 
    UMLPackagePath ( "CIM::System::SystemResources" ), 
    Description ( 
       "Personal Computer architecture Memory Mapped I/O. This class "
       "addresses both memory and port I/O resources. The property, "
       "MappedResource, defines whether memory or I/O is mapped (and "
       "for I/O whether the mapping is to a memory or a port space)." )]
class CIM_MemoryMappedIO : CIM_SystemResource {

      [Key, Description ( 
          "The scoping ComputerSystem\'s CreationClassName." ), 
       MaxLen ( 256 ), 
       Propagated ( "CIM_ComputerSystem.CreationClassName" )]
   string CSCreationClassName;

      [Key, Description ( "The scoping ComputerSystem\'s Name." ), 
       MaxLen ( 256 ), 
       Propagated ( "CIM_ComputerSystem.Name" )]
   string CSName;

      [Key, Description ( 
          "CreationClassName indicates the name of the class or the "
          "subclass used in the creation of an instance. When used "
          "with the other key properties of this class, this "
          "property allows all instances of this class and its "
          "subclasses to be uniquely identified." ), 
       MaxLen ( 256 )]
   string CreationClassName;

      [Key, Description ( 
          "A part of the object\'s key value, the starting address "
          "of memory mapped I/O." ), 
       MappingStrings { "MIF.DMTF|Memory Mapped I/O|001.1" }]
   uint64 StartingAddress;

      [Description ( "Ending address of memory mapped I/O." ), 
       MappingStrings { "MIF.DMTF|Memory Mapped I/O|001.2" }]
   uint64 EndingAddress;

      [Description ( 
          "Type of memory mapped I/O. MappedResource defines "
          "whether memory or I/O is mapped, and for I/O, whether "
          "the mapping is to a memory or a port space." ), 
       ValueMap { "0", "1", "2", "3" }, 
       Values { "Other", "Mapped Memory", 
          "I/O Mapped to Memory Space", "I/O Mapped to Port Space" }]
   uint16 MappedResource;


};
